{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Cover","Kräfte","Tragwerke","Biegeträger"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":20,"n_cols":3,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Excel + VBA"]
[]
[]
[null,"Kapitel",2]
[null,"Thema","Berechnungen aus der Statik"]
[]
[null,"Inhalt","Kräfte im Raum"]
[null,null,"Kräfte in Tragwerken"]
[null,null,"Biegeträger"]
[]
[]
[]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2017-03-01"]
[null,"Version","5.0"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Kräfte","index":1,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,0,0,2],[0,3,0,5]]}
["Angriffspunkt",null,null,"Kraftkomponenten",null,null,"Resultierende Kraft",7.0710678118654755]
["x","y","z","x","y","z","Resultierendes Moment",14.035668847618199]
[3,0,0,0,3,0,"Ortsvektor a(x)",-0.26]
[0,1,0,0,0,4,"Ortsvektor a(y)",-0.57999999999999996]
[0,0,2,5,0,0,"Ortsvektor a(z)",0.76]
[null,null,null,null,null,null,"Moment Mf(x)",8.6]
[5,3,4,4,10,9,"Moment Mf(y)",5.16]
[null,null,null,null,null,null,"Moment Mf(z)",6.88]

{"sheet":"Tragwerke","index":2,"n_rows":17,"n_cols":8,"rows_kept":17,"cut":false,"hidden":false,"merged":[[0,1,0,2],[0,3,0,4],[0,5,0,6]]}
[null,"Stabkräfte",null,"Bekannte Kräfte am Knoten",null,"Result. + unbek. Kräfte am Knoten"]
["Stab-Nr.","Winkel [Grad]","Kraft [N]","Winkel [Grad]","Kraft [N]","Winkel [Grad]","Kraft [N]","Stab Nr."]
[1,126.9,-11254.44285348596,26.57,-32948.19,233.09364250926274,33761.670817812628]
[2,180,6757.4021592902973,306.87,15323.78,233.13,-33761.670817812628,15]
[3,153.43,-10981.236322810855]
[4,233.13,5114.6697469437622]
[5,113.2,-4451.7305600408536]
[6,180,11579.934352760352]
[7,180,-15434.145053116812]
[8,246.8,9795.6669074271158]
[9,113.2,-9795.6922863876134]
[10,180,19297.794457700835]
[11,206.57,-32948.18721771385]
[12,246.8,25829.676943904306]
[13,126.87,15323.778565281136]
[14,180,20278.87670269977]
[15,233.13,-33761.670817812628]

{"sheet":"Biegeträger","index":3,"n_rows":22,"n_cols":3,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["Stelle\nx [cm]","Moment\nM [Ncm]","Biegung\nx [cm]"]
[0,1200000,0]
[2,1102000,-1.8519999999999999E-3]
[4,1008000,-7.2040000000000003E-3]
[6,918000,-1.5757E-2]
[8,832000,-2.7224999999999999E-2]
[10,750000,-4.1335999999999998E-2]
[12,672000,-5.7828999999999998E-2]
[14,598000,-7.6455999999999996E-2]
[16,528000,-9.6981999999999999E-2]
[18,462000,-0.119186]
[20,400000,-0.14285700000000001]
[22,342000,-0.167799]
[24,288000,-0.193829]
[26,238000,-0.220773]
[28,192000,-0.248474]
[30,150000,-0.27678599999999998]
[32,112000,-0.30557499999999999]
[34,78000,-0.33472000000000002]
[36,48000,-0.36411399999999999]
[38,22000,-0.39366200000000001]
[40,0,-0.42327999999999999]