{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Geschweißter Biegeträger","Monte-Carlo"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":20,"n_cols":3,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Excel + VBA"]
[]
[]
[null,"Kapitel",4]
[null,"Thema","Festigkeitsberechnungen"]
[]
[null,"Inhalt","Hauptspannungen eines zusammengesetzten Biegeträgers"]
[null,null,"Anwendung der Monte-Carlo-Methode"]
[]
[]
[]
[]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2017-03-01"]
[null,"Version","5.0"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Geschweißter Biegeträger","index":1,"n_rows":14,"n_cols":9,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,2,0,4],[0,6,0,8]]}
["FN [N]",5000,"Maße",null,null,"Schwerpkt.","Schweißnähte"]
["FQ [N]",1000,"b [mm]","h [mm]","a [mm]","e [mm]","σb [N/cm²]","τa [N/cm²]","σh [N/cm²]"]
["Mb [Nm]",500,600,100,0,50]
[null,null,200,200,5,200,1.417099669343411,8.5025980160604622,11.532167888197602]
["H [mm]",450,100,100,4,350,-2.2673594709494571,12.753897024090698,13.567700565629492]
["e [mm]",176.92307692307693,400,50,4,425,-4.1095890410958926,36.56117146906,36.429691137908556]
["A [cm²]",1300]
["I [cm^4]",271410.25641025632]
["σz [N/cm²]",3.8461538461538463]
["τa [N/cm²]",0.76923076923076927]
["σb1 [N/cm²]",3.2593292394898454]
["σb2 [N/cm²]",-5.030703826169109]
["σh1 [N/cm²]",7.1878052900515303]
["σh2 [N/cm²]",0.37855230674493767]

{"sheet":"Monte-Carlo","index":2,"n_rows":12,"n_cols":9,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,2,0,8]]}
["F [N]",20000,"Auswertung"]
["E [N/cm²]",21000000,"n","h [cm]","l [cm]","σ [N/cm²]","I [cm^4]","f [cm]","V [cm^3]"]
["k ",0.25,2,22.856431007385254,151.26871466636658,6080.8613763796047,5685.8111480353155,0.1932610637439369,19756.315789161876]
["σzul [N/cm²]",10000,82,22.11226749420166,159.62004065513611,7086.4514517170892,4980.71716210866,0.25921481370856875,19511.649443506583]
["fzul [cm]",0.3,298,22.302220344543457,156.60404562950134,6776.4136355678038,5154.0801968524256,0.23656321074612044,19473.283677346317]
["hmin [cm]",22,321,22.055662631988525,153.64812016487122,6873.9783232757118,4929.9124073768326,0.23357803294289836,18685.618599493799]
["hmax [cm]",26,587,22.210750102996826,150.14644265174866,6577.5870900757427,5070.0432710705945,0.21194487609522775,18517.463932956201]
["lmin [cm]",150,850,22.00423526763916,152.09745764732361,6852.4259785848199,4884.0925128426979,0.22870277218383728,18410.878965231983]
["lmax [cm]",250,1476,22.085283279418945,150.92608332633972,6725.0670199774595,4956.4491991138148,0.22019714942058771,18403.916697503926]
["n",100000,1798,22.072939872741699,150.31375288963318,6709.0250676090609,4945.3778993874548,0.21801487011860207,18308.766551471512]
[null,null,3054,22.040060997009277,150.14294981956482,6731.4373032505509,4915.9780047214408,0.21857191000021373,18233.52080755289]
[null,null,32629,22.013878345489502,150.38545727729797,6766.3956987025804,4892.6597096117648,0.22067948269896781,18219.605686591]