{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Rotation","Strömung"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":20,"n_cols":3,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Excel + VBA"]
[]
[]
[null,"Kapitel",8]
[null,"Thema","Berechnungen aus der Strömungslehre"]
[]
[null,"Inhalt","Rotation von Flüssigkeiten"]
[null,null,"Laminare Strömung in zylindrischen Rohren"]
[]
[]
[]
[]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2017-03-01"]
[null,"Version","5.0"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Rotation","index":1,"n_rows":3,"n_cols":1,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Gefäßradius r [m]"]
["Spiegelhöhe y0 [m]"]
["Winkelgeschwindigkeit w [1/s]"]

{"sheet":"Strömung","index":2,"n_rows":9,"n_cols":1,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["Rohrlänge l [m]"]
["Rohrinnenradius r0 [m]"]
["Druckdifferenz p [N/cm²]"]
["Flüssigkeitsdichte [kg/dm³]"]
["Dynamische Zähigkeit [Ns/m²]"]
["Neigungswinkel [Grad]"]
[]
["Mittl.Strömungsgeschw. vm [m/s]"]
["Volumenstrom Q [m³/s]"]