{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Gleichstrom","Wechselstrom"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":20,"n_cols":3,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Excel + VBA"]
[]
[]
[null,"Kapitel",10]
[null,"Thema","Berechnungen aus der Elektrotechnik"]
[]
[null,"Inhalt","Spannungen und Ströme in Gleichstromleitungen"]
[null,null,"Rechnen mit komplexen Zahlen"]
[null,null,"Gesamtwiderstand einer Wechselstromschaltung"]
[]
[]
[]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2017-03-01"]
[null,"Version","5.0"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Gleichstrom","index":1,"n_rows":6,"n_cols":8,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["Minimale Leitungslänge [m]",null,null,"Leitungs-",null,"Spannungs-","Leistungs"]
["Maximale Leitungslänge [m]",null,null,"Länge","Widerst.","Verlust","Verlust"]
["Leitungsdurchmesser [mm]",null,null,"[m]","[Ohm]","[V]","[W]","[%]"]
["Spez. Widerstand [Ohm mm²/m]"]
["Elektr. Spannung [V]"]
["Elektr. Strom [A]"]

{"sheet":"Wechselstrom","index":2,"n_rows":3,"n_cols":5,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Ohmscher Widerstand R [Ohm]",null,null,"w [1/s]","|Z|"]
["Kapazitiver Widerstand C [F]"]
["Induktiver Widerstand L [H]"]