{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Werkstoff-Sammlung","Tabelle1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":23,"n_cols":3,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Excel + VBA"]
[]
[]
[null,"Kapitel",5]
[null,"Thema","Festigkeitsberechnungen"]
[]
[null,"Inhalt","Werkstoffsammlung"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2020-09-01"]
[null,"Version","6.0"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Werkstoff-Sammlung","index":1,"n_rows":11,"n_cols":21,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Kennung","Material","Mechanische\nEigenschaften","E-Modul\n[N/mm^2]","Zugfestigkeit\n[N/mm^2]","Druckfestigkeit\n[N/mm^2]","Biege-Zugfestigkeit\n[N/mm^2]","Querdezhnungszahl\n[-]","etc.","Physikalische\nEigenschaften","Dichte\n[g/cm^3]","Thermische\nLeitfähigkeit\n[W/mK]","spezifische\nWärmekapazität\n[J/gK]","Wärmedehnzahl\n[10^-6 K^-1]","spezifischer\nelektrischer\nWiderstand","etc.","Umwelteinflüsse","Oxidation","Korrosion","Verschleiss","etc."]
[null,"Feste Werkstoffe"]
["w","Stahl",null,210000,380,380,410,0.28000000000000003,null,null,7.8,0.45,0.45,12]
["w","Aluminium",null,66000,290,85,310,0.34,null,null,2.7,0.9,0.9,23]
["w","Holz",null,10000,50,45,35,0.24,null,null,0.7,0.13,2.1,5]
["w","Glas",null,62000,65,650,75,0.25,null,null,2.5,9,0.8,9]
[null,"Flüssige Werkstoffe"]
["w","Benzol",null,0,null,null,null,0,null,null," ",null,1.738]
["w","Ethanol",null,0,null,null,null,0,null,null,null,null,2.4500000000000002]
["w","Motorenöl",null,0,null,null,null,0,null,null,null,null,1.86]
["w","Parafin",null,0,null,null,null,0,null,null,null,null,2.16]

{"sheet":"Tabelle1","index":2,"n_rows":6,"n_cols":7,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["Material","Mechanische\nEigenschaften","E-Modul\n[N/mm^2]","Zugfestigkeit\n[N/mm^2]","Druckfestigkeit\n[N/mm^2]","Biege-Zugfestigkeit\n[N/mm^2]","Querdezhnungszahl\n[-]"]
[]
["Stahl",null,210000,380,380,410,0.28000000000000003]
["Aluminium",null,66000,290,85,310,0.34]
["Holz",null,10000,50,45,35,0.24]
["Glas",null,62000,65,650,75,0.25]