{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Cover","Fügen"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":20,"n_cols":3,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Excel + VBA"]
[null,"für Ingenieure"]
[]
[]
[null,"Kapitel",12]
[null,"Thema","Berechnungen aus der Fertigungstechnik"]
[]
[null,"Inhalt","Fügen"]
[]
[]
[]
[]
[null,"Version","7.0"]
[null,"Autor","Harald Nahrstedt"]
[null,"Letzte Bearbeitung","2023-03-04"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Fügen","index":1,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Äußerer Durchmesser da",200,"mm"]
["Innerer Durchmesser di",80,"mm"]
["Fügelänge l",220,"mm"]
["zul. Druckspannung außen Szul,a",630,"N/mm^2"]
["zul. Druckspannung innen Szul,i",480,"N/mm^2"]
["Haftbeiwert n",0.2,"-"]
[]
["opt. Fugendurchmesser df",144.50805664062497,"mm"]
["vorhandene Fugenpressung",166.44342483267067,"N/mm^2"]
["übertragbare Axialkraft",3324.7644826706232,"kN"]
["übertragbares Drehmoment",240.22762708925234,"kNm"]