{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Cover","Schneckentrieb"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":20,"n_cols":3,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Excel + VBA"]
[null,"für Ingenieure"]
[]
[]
[null,"Kapitel",13]
[null,"Thema","Berechnungen aus der Antriebstechnik"]
[]
[null,"Inhalt","Lagerreaktionen"]
[]
[]
[]
[]
[null,"Version","7.0"]
[null,"Autor","Harald Nahrstedt"]
[null,"Letzte Bearbeitung","2023-03-04"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Schneckentrieb","index":1,"n_rows":40,"n_cols":3,"rows_kept":40,"cut":false,"hidden":false,"merged":[]}
["E-Modul",208000,"N/mm^2"]
["Kraftkomponente in x-Achse",2100,"N"]
["Kraftkomponente in y-Achse",1400,"N"]
["Kraftkomponente in z-Achse",1860,"N"]
["Lagerabstand x",1850,"mm"]
["Lagerabstand z",1460,"mm"]
["Wälzradius Schnecke",208.6,"mm"]
["Wälzradius Schneckenrad",448.8,"mm"]
["Wellendurchmesser",130,"mm"]
[]
["Lagerbelastungen:"]
["1. Lager"]
["   y-Komponente",463.21081081081081,"N"]
["   z-Komponente",930,"N"]
["   Resultierende",1038.9726922551954,"N"]
["2. Lager"]
["   y-Komponente",936.78918918918919,"N"]
["   z-Komponente",930,"N"]
["   Resultierende",1320.0280243168093,"N"]
["3. Lager"]
["   x-Komponente",1050,"N"]
["   y-Komponente",1271.7589041095891,"N"]
["   Resultierende",1649.2030530477512,"N"]
["4. Lager"]
["   x-Komponente",1050,"N"]
["   y-Komponente",128.24109589041095,"N"]
["   Resultierende",1057.8023344061846,"N"]
["Biegemomente:"]
["   z-Komponente",647800.04109589045,"Nmm"]
["   y-Komponente",860250,"Nmm"]
["   Resultierende",1076882.0528469388,"Nmm"]
["Spannungen:"]
["   Biegung",4.992735449592157,"N/mm^2"]
["   Zug/Druck",0.1582133315035836,"N/mm^2"]
["   Torsion",0.89943061934160329,"N/mm^2"]
["   Vergleichsspannung",5.3056784885149364,"N/mm^2"]
["Durchbiegung:"]
["   y-Komponente",3.1663995254936579E-2,"mm"]
["   z-Komponente",4.2067879410130023E-2,"mm"]
["   Resultierende",5.2652778403137354E-2,"mm"]