{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Cover","Tabelle1"],"not_rendered":{"charts":2,"images":0,"macros":0,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":22,"n_cols":3,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Excel + VBA"]
[null,"für Ingenieure"]
[null,"8. Auflage"]
[]
[]
[null,"Kapitel",17]
[null,"Thema","Solarkollektor"]
[]
[null,"Inhalt","Berechnung des Energiegewinns"]
[]
[]
[]
[]
[]
[null,"Version","1.0"]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2025-02-21"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Tabelle1","index":1,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
["ksum",1000," Watt/m2"]
["ASK",2,"m2"]
["n",4]
["c",3.6,"kJ/kg"]
["ΔT",20,"Grad"]
[]
["t [s]","Esol [kWh]","m [kg]"]
[0,{"$f":"ks*n*As*A8","v":0},{"$f":"B8/(cg*dT)","v":0}]
[200,1600000,{"$f":"B9/(cg*dT)/1000","v":22.222222222222221}]
[400,3200000,44.444444444444443]
[600,4800000,66.666666666666671]
[800,6400000,88.888888888888886]
[1000,8000000,111.11111111111111]
[1200,9600000,133.33333333333334]
[1400,11200000,155.55555555555557]
[1600,12800000,177.77777777777777]
[1800,14400000,200]
[2000,16000000,222.22222222222223]
[2200,17600000,244.44444444444443]
[2400,19200000,266.66666666666669]
[2600,20800000,288.88888888888886]
[2800,22400000,311.11111111111114]
[3000,24000000,333.33333333333331]
[3200,25600000,355.55555555555554]
[3400,27200000,377.77777777777777]
[3600,28800000,400]
[3800,30400000,422.22222222222223]
[4000,32000000,444.44444444444446]