{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Wasserkraftwerk","Speicherkraftwerk"],"not_rendered":{"charts":2,"images":0,"macros":0,"external_links":0,"defined_names":10,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":21,"n_cols":3,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Excel + VBA"]
[null,"für Ingenieure"]
[null,"8. Auflage"]
[]
[]
[null,"Kapitel",17]
[null,"Thema","Pumpspeicherwerk"]
[]
[null,"Inhalt","Beziehug zwischen Energiebedarf"]
[null,null,"und Volumenumsatz"]
[]
[]
[]
[null,"Version","1.0"]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2025-02-21"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Wasserkraftwerk","index":1,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["ηSpeicher",0.89,null,"EEleR  [MWh]","EPot [MWh]","EEleP [MWh]","V [km3]","Δh [m]"]
["ηRückgewinnung",0.85,null,10,{"$f":"D2/EtaR","v":11.764705882352942},{"$f":"E2/EtaS","v":13.218770654329148},{"$f":"100000*E2/RohW/9.81/Hmit*3.6/9.81","v":0.44009411412630595},{"$f":"G2/Aob","v":4.1130291039841678E-2}]
["ρWasser",1000,"kg/m3",20,23.529411764705884,26.437541308658297,0.88018822825261189,8.2260582079683356E-2]
["hmittel",100,"m",30,35.294117647058826,39.656311962987445,1.3202823423789176,0.12339087311952501]
["AO",10.7,"km2",40,47.058823529411768,52.875082617316593,1.7603764565052238,0.16452116415936671]
[null,null,null,50,58.82352941176471,66.093853271645742,2.2004705706315297,0.20565145519920841]
["ηGesamt",{"$f":"EtaS*EtaR","v":0.75649999999999995},null,60,70.588235294117652,79.31262392597489,2.6405646847578352,0.24678174623905003]
[null,null,null,70,82.352941176470594,92.531394580304038,3.0806587988841416,0.28791203727889175]
[null,null,null,80,94.117647058823536,105.75016523463319,3.5207529130104476,0.32904232831873342]
[null,null,null,90,105.88235294117648,118.96893588896233,3.9608470271367535,0.37017261935857509]
[null,null,null,100,117.64705882352942,132.18770654329148,4.4009411412630595,0.41130291039841682]
[null,null,null,110,129.41176470588235,145.4064771976206,4.8410352553893645,0.45243320143825838]
[null,null,null,120,141.1764705882353,158.62524785194978,5.2811293695156705,0.49356349247810005]
[null,null,null,130,152.94117647058823,171.8440185062789,5.7212234836419764,0.53469378351794172]
[null,null,null,140,164.70588235294119,185.06278916060808,6.1613175977682832,0.57582407455778351]
[null,null,null,150,176.47058823529412,198.2815598149372,6.6014117118945883,0.61695436559762507]
[null,null,null,160,188.23529411764707,211.50033046926637,7.0415058260208951,0.65808465663746685]
[null,null,null,170,200,224.71910112359549,7.4815999401472002,0.69921494767730852]
[null,null,null,180,211.76470588235296,237.93787177792467,7.921694054273507,0.74034523871715019]
[null,null,null,190,223.52941176470588,251.15664243225379,8.3617881683998103,0.78147552975699164]
[null,null,null,200,235.29411764705884,264.37541308658297,8.8018822825261189,0.82260582079683364]

{"sheet":"Speicherkraftwerk","index":2,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["η",0.85,null,"h [m]","EPot [MWh]"]
["ρWasser",1000,"kg/m3",100,{"$f":"Eta*Roh*9.81*hw*Vol/3600/1000000","v":2.3162500000000001}]
["V",10000,"m3",110,2.5478749999999999]
[null,null,null,120,2.7795000000000001]
[null,null,null,130,3.0111249999999998]
[null,null,null,140,3.24275]
[null,null,null,150,3.4743750000000002]
[null,null,null,160,3.706]
[null,null,null,170,3.9376250000000002]
[null,null,null,180,4.1692499999999999]
[null,null,null,190,4.4008750000000001]
[null,null,null,200,4.6325000000000003]
[null,null,null,210,4.8641249999999996]
[null,null,null,220,5.0957499999999998]
[null,null,null,230,5.327375]
[null,null,null,240,5.5590000000000002]
[null,null,null,250,5.7906250000000004]
[null,null,null,260,6.0222499999999997]
[null,null,null,270,6.2538749999999999]
[null,null,null,280,6.4855]
[null,null,null,290,6.7171250000000002]
[null,null,null,300,6.9487500000000004]