{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Cover","Geschweißter Biegeträger"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":23,"n_cols":3,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Excel + VBA"]
[]
[]
[null,"Kapitel",5]
[null,"Thema","Festigkeitsberechnungen"]
[]
[null,"Inhalt","Hauptspannungen eines zusammengesetzten Biegeträgers"]
[null,null,"Anwendung der Monte-Carlo-Methode"]
[]
[]
[]
[]
[]
[]
[]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2020-09-01"]
[null,"Version","6.0"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Geschweißter Biegeträger","index":1,"n_rows":14,"n_cols":9,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,2,0,4],[0,6,0,8]]}
["FN [N]",5000,"Maße",null,null,"Schwerpkt.","Schweißnähte"]
["FQ [N]",1000,"b [mm]","h [mm]","a [mm]","e [mm]","σb [N/cm²]","τa [N/cm²]","σh [N/cm²]"]
["Mb [Nm]",500,600,100,0,50]
[null,null,200,200,5,200,-1.062648735867471,2.0650663692971093E-2,2.7836583079362969]
["H [mm]",450,100,100,4,350,1.7337953058890314,3.7429327943510109E-2,5.5802002101658017]
["e [mm]",176.92307692307693,400,50,4,425,3.1320173267672828,0.10712531790728755,6.9798153186775407]
["A [cm²]",1300]
["I [cm^4]",357597.43589743588]
["σz [N/cm²]",3.8461538461538463]
["τa [N/cm²]",0.76923076923076927]
["σb1 [N/cm²]",3.8311283372064082]
["σb2 [N/cm²]",-2.460870756745722]
["σh1 [N/cm²]",7.7535972098335044]
["σh2 [N/cm²]",1.7277590673947905]