{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Cover","Zeiten"],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":1,"defined_names":10,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":20,"n_cols":3,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Excel + VBA"]
[]
[]
[null,"Kapitel",17]
[null,"Thema","Windrad"]
[]
[null,"Inhalt","Berechnung des Energiegewinns"]
[]
[]
[]
[]
[]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2022-09-16"]
[null,"Version","7.0"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Zeiten","index":1,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["cp",0.45]
["dR",100,"m","AR",{"$f":"dr^2*PI()/4","v":7853.981633974483},"m2"]
["δL",1.1399999999999999,"kg/m3"]
["vW",12,"m/s"]
[]
["t [h]","Ewin [Mio kWh]"]
[0,{"$f":"cp*dl*AR*vw^3*A7/2000000000","v":0}]
[500,{"$f":"cp*dl*AR*vw^3*A8/2000000000","v":1.7405679937948892}]
[1000,{"$f":"cp*dl*AR*vw^3*A9/2000000000","v":3.4811359875897785}]
[1500,{"$f":"cp*dl*AR*vw^3*A10/2000000000","v":5.2217039813846675}]
[2000,{"$f":"cp*dl*AR*vw^3*A11/2000000000","v":6.962271975179557}]
[2500,{"$f":"cp*dl*AR*vw^3*A12/2000000000","v":8.7028399689744447}]
[3000,{"$f":"cp*dl*AR*vw^3*A13/2000000000","v":10.443407962769335}]
[3500,{"$f":"cp*dl*AR*vw^3*A14/2000000000","v":12.183975956564224}]
[4000,{"$f":"cp*dl*AR*vw^3*A15/2000000000","v":13.924543950359114}]
[4500,{"$f":"cp*dl*AR*vw^3*A16/2000000000","v":15.665111944154003}]
[5000,{"$f":"cp*dl*AR*vw^3*A17/2000000000","v":17.405679937948889}]
[5500,{"$f":"cp*dl*AR*vw^3*A18/2000000000","v":19.146247931743783}]
[6000,{"$f":"cp*dl*AR*vw^3*A19/2000000000","v":20.88681592553867}]
[6500,{"$f":"cp*dl*AR*vw^3*A20/2000000000","v":22.62738391933356}]
[7000,{"$f":"cp*dl*AR*vw^3*A21/2000000000","v":24.367951913128447}]
[7500,{"$f":"cp*dl*AR*vw^3*A22/2000000000","v":26.108519906923338}]
[8000,{"$f":"cp*dl*AR*vw^3*A23/2000000000","v":27.849087900718228}]
[8500,{"$f":"cp*dl*AR*vw^3*A24/2000000000","v":29.589655894513115}]
[9000,{"$f":"cp*dl*AR*vw^3*A25/2000000000","v":31.330223888308005}]