{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Cover","Tabelle1"],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":2,"defined_names":13,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":20,"n_cols":3,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Excel + VBA"]
[]
[]
[null,"Kapitel",17]
[null,"Thema","Erdwärme"]
[]
[null,"Inhalt","Beziehung zwischen Leistungszahl"]
[null,null,"und Temperaturdifferenz"]
[]
[]
[]
[]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2022-09-16"]
[null,"Version","7.0"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Tabelle1","index":1,"n_rows":22,"n_cols":3,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["T0",273.14999999999998,"oK"]
["ΔTV",5,"oK"]
["η",0.6]
[]
["ΔTK","ε"]
[10,{"$f":"fN*((T0+A6)/((T0+A6)-(T0+TV)))","v":33.977999999999994}]
[15,17.288999999999998]
[20,11.725999999999999]
[25,8.9444999999999997]
[30,7.275599999999999]
[35,6.1629999999999994]
[40,5.3682857142857134]
[45,4.7722499999999997]
[50,4.3086666666666664]
[55,3.9377999999999997]
[60,3.634363636363636]
[65,3.3815]
[70,3.1675384615384612]
[75,2.9841428571428565]
[80,2.8252000000000002]
[85,2.6861249999999997]
[90,2.5634117647058825]