{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Cover","Gleichstrom"],"not_rendered":{"charts":2,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":21,"n_cols":3,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Excel + VBA"]
[null,"für Ingenieure"]
[null,"8. Auflage"]
[]
[]
[null,"Kapitel",10]
[null,"Thema","Elektrotechnik"]
[]
[null,"Inhalt","Spannungen und Ströme in Gleichstromleitungen"]
[]
[]
[]
[]
[null,"Version","1.0"]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2025-02-21"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Gleichstrom","index":1,"n_rows":14,"n_cols":8,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["Minimale Leitungslänge [m]",100,null,"Leitungs-",null,"Spannungs-","Leistungs"]
["Maximale Leitungslänge [m]",600,null,"Länge","Widerst.","Verlust","Verlust"]
["Leitungsdurchmesser [mm]",6,null,"[m]","[Ohm]","[V]","[W]","[%]"]
["Spez. Widerstand [Ohm mm²/m]",0.02,null,100,7.0735531469682686E-2,1.131768503514923,9.0541480281193838,0.1131768503514923]
["Elektr. Spannung [V]",1000,null,150,0.10610329720452402,1.6976527552723844,13.581222042179075,0.16976527552723844]
["Elektr. Strom [A]",8,null,200,0.14147106293936537,2.2635370070298459,18.108296056238768,0.22635370070298461]
[null,null,null,250,0.17683882867420669,2.8294212587873071,22.635370070298457,0.28294212587873069]
[null,null,null,300,0.21220659440904804,3.3953055105447687,27.16244408435815,0.33953055105447688]
[null,null,null,350,0.24757436014388937,3.9611897623022299,31.689518098417839,0.39611897623022296]
[null,null,null,400,0.28294212587873074,4.5270740140596919,36.216592112477535,0.45270740140596921]
[null,null,null,450,0.31830989161357204,5.0929582658171526,40.743666126537221,0.50929582658171524]
[null,null,null,500,0.35367765734841339,5.6588425175746142,45.270740140596914,0.56588425175746138]
[null,null,null,550,0.38904542308325474,6.2247267693320758,49.797814154656606,0.62247267693320762]
[null,null,null,600,0.42441318881809609,6.7906110210895374,54.324888168716299,0.67906110210895376]