{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Cover","Temperaturverteilung"],"not_rendered":{"charts":1,"images":0,"macros":1,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":21,"n_cols":3,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Algorithmen"]
[null,"für Ingenieure"]
[]
[]
[null,"Kapitel",3]
[null,"Thema","Lösen linearer Gleichungssysteme"]
[]
[null,"Inhalt","Temperaturverteilung"]
[null,null," "]
[]
[]
[]
[]
[null,"Version","1.0"]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2025-06-15"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Temperaturverteilung","index":1,"n_rows":24,"n_cols":18,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
[4,-1,0,0,0,-1,0,0,0,0,0,0,0,0,0,24,null,16.031334114861679]
[-1,4,-1,0,0,0,-1,0,0,0,0,0,0,0,0,18,null,20.313016551653927]
[0,-1,4,-1,0,0,0,-1,0,0,0,0,0,0,0,24,null,25.17001812620369]
[0,0,-1,4,-1,0,0,0,-1,0,0,0,0,0,0,36,null,31.146142845649791]
[0,0,0,-1,4,0,0,0,0,-1,0,0,0,0,0,84,null,35.960112582770584]
[-1,0,0,0,0,4,-1,0,0,0,-1,0,0,0,0,22,null,19.812319907792787]
[0,-1,0,0,0,-1,4,-1,0,0,0,-1,0,0,0,0,null,22.050713965550358]
[0,0,-1,0,0,0,-1,4,-1,0,0,0,-1,0,0,0,null,25.220913107511045]
[0,0,0,-1,0,0,0,-1,4,-1,0,0,0,-1,0,0,null,27.454440673624894]
[0,0,0,0,-1,0,0,0,-1,4,0,0,0,0,-1,30,null,28.694307485432542]
[0,0,0,0,0,-1,0,0,0,0,4,-1,0,0,0,34,null,19.167231550759116]
[0,0,0,0,0,0,-1,0,0,0,-1,4,-1,0,0,24,null,22.856606295243676]
[0,0,0,0,0,0,0,-1,0,0,0,-1,4,-1,0,32,null,26.208479664665237]
[0,0,0,0,0,0,0,0,-1,0,0,0,-1,4,-1,24,null,24.756399255906206]
[0,0,0,0,0,0,0,0,0,-1,0,0,0,-1,4,32,null,21.362676685334687]
[]
[]
[]
[]
[12,12,18,24,36,42,42]
[12,16.031334114861679,20.313016551653927,25.17001812620369,31.146142845649791,35.960112582770584,42]
[22,19.812319907792787,22.050713965550358,25.220913107511045,27.454440673624894,28.694307485432542,30]
[18,19.167231550759116,22.856606295243676,26.208479664665237,24.756399255906206,21.362676685334687,16]
[17,16,24,32,24,16,16]