{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Cover","Gauss-Biegung"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":21,"n_cols":3,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Algorithmen"]
[null,"für Ingenieure"]
[]
[]
[null,"Kapitel",6]
[null,"Thema","Differenzenverfahren"]
[]
[null,"Inhalt","Einseitig eingespannter Biegeträger"]
[]
[]
[]
[]
[]
[null,"Version","1.0"]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2025-06-16"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Gauss-Biegung","index":1,"n_rows":11,"n_cols":6,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[7,-4,1,0,null,0]
[-4,6,-4,1,null,0]
[1,-4,5,-2,null,0]
[0,2,-4,2,null,0.03]
[]
[7,-4,1,0,null,0]
[-2.2204460492503131E-16,3.7142857142857144,-3.4285714285714288,1,null,0]
[-1.4945309946877108E-16,5.377642775528102E-17,1.6923076923076916,-1.0769230769230769,null,0]
[-7.0650556112510047E-17,9.5330940111634558E-17,-4.9656459499836103E-17,9.0909090909090648E-2,null,0.03]
[]
[3.000000000000012E-2,0.10500000000000038,0.21000000000000069,0.33000000000000096,null,0]