{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["Cover","Quicksort","Produkt","P001","P002","P003","P004","S-P001"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":21,"n_cols":3,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Algorithmen"]
[null,"für Ingenieure"]
[]
[]
[null,"Kapitel",8]
[null,"Thema","Listenstrukturen"]
[]
[null,"Inhalt","Quicksort"]
[null,null,"Stücklisten"]
[]
[]
[]
[]
[null,"Version","1.0"]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2025-06-16"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Quicksort","index":1,"n_rows":100,"n_cols":1,"rows_kept":100,"cut":false,"hidden":false,"merged":[]}
[1.1522650718688965E-2]
[1.6518712043762207E-2]
[2.4931430816650391E-2]
[2.5494694709777832E-2]
[3.3299684524536133E-2]
[3.8365185260772705E-2]
[5.9280633926391602E-2]
[6.5847277641296387E-2]
[9.9478065967559814E-2]
[0.10071909427642822]
[0.10530835390090942]
[0.11747163534164429]
[0.13827145099639893]
[0.13957411050796509]
[0.14448052644729614]
[0.15985077619552612]
[0.1637192964553833]
[0.19119715690612793]
[0.22751349210739136]
[0.23763525485992432]
[0.23870664834976196]
[0.2489740252494812]
[0.29596096277236938]
[0.29937964677810669]
[0.31422555446624756]
[0.31466203927993774]
[0.32504290342330933]
[0.33776432275772095]
[0.34095704555511475]
[0.35643970966339111]
[0.3607754111289978]
[0.37444388866424561]
[0.38197368383407593]
[0.38271617889404297]
[0.38421010971069336]
[0.39950460195541382]
[0.39957964420318604]
[0.40727168321609497]
[0.42036032676696777]
[0.45669388771057129]
[0.46675485372543335]
[0.49467313289642334]
[0.4966997504234314]
[0.53113853931427002]
[0.54738545417785645]
[0.55050063133239746]
[0.552165687084198]
[0.56138688325881958]
[0.60028964281082153]
[0.60210424661636353]
[0.60784697532653809]
[0.61230683326721191]
[0.64613664150238037]
[0.64859622716903687]
[0.65785723924636841]
[0.66003221273422241]
[0.66381514072418213]
[0.66481590270996094]
[0.66643023490905762]
[0.67172956466674805]
[0.67876613140106201]
[0.67921972274780273]
[0.6860203742980957]
[0.69449561834335327]
[0.69885045289993286]
[0.72814071178436279]
[0.73444610834121704]
[0.73719120025634766]
[0.75992792844772339]
[0.76262181997299194]
[0.76416736841201782]
[0.77329659461975098]
[0.7750585675239563]
[0.81096428632736206]
[0.81356459856033325]
[0.81663703918457031]
[0.81818819046020508]
[0.8198285698890686]
[0.83709579706192017]
[0.84938186407089233]
[0.85190737247467041]
[0.85470682382583618]
[0.85500591993331909]
[0.87056452035903931]
[0.8718944787979126]
[0.87673491239547729]
[0.87683486938476563]
[0.88948172330856323]
[0.8931611180305481]
[0.89408910274505615]
[0.93250364065170288]
[0.93407714366912842]
[0.9436652660369873]
[0.95680826902389526]
[0.9708791971206665]
[0.97694462537765503]
[0.98584622144699097]
[0.9859541654586792]
[0.99039936065673828]
[0.99628567695617676]

{"sheet":"Produkt","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"P001","index":3,"n_rows":6,"n_cols":6,"rows_kept":6,"cut":false,"hidden":false,"merged":[[0,0,0,5]]}
["P001- Baugruppe"]
["Stufe","Pos.Nr.","Menge","Bezeichnung","Baugruppe","Material"]
["1","1","1","BG1","P002"]
["1","2","1","BG2","P003"]
["1","3","2","ET3",null,"1 m"]
["1","4","1","ET4",null,"2 kg"]

{"sheet":"P002","index":4,"n_rows":4,"n_cols":6,"rows_kept":4,"cut":false,"hidden":false,"merged":[[0,0,0,5]]}
["P002- Baugruppe"]
["Stufe","Pos.Nr.","Menge","Bezeichnung","Baugruppe","Material"]
[1,1,1,"ET1",null,"1 kg"]
[1,2,2,"ET2",null,"1,5 m"]

{"sheet":"P003","index":5,"n_rows":5,"n_cols":6,"rows_kept":5,"cut":false,"hidden":false,"merged":[[0,0,0,5]]}
["P003- Baugruppe"]
["Stufe","Pos.Nr.","Menge","Bezeichnung","Baugruppe","Material"]
[1,1,2,"ET1",null,"1 kg"]
[1,2,3,"ET3",null,"2 kg"]
[1,3,1,"BG3","P004"]

{"sheet":"P004","index":6,"n_rows":5,"n_cols":6,"rows_kept":5,"cut":false,"hidden":false,"merged":[[0,0,0,5]]}
["P004- Baugruppe"]
["Stufe","Pos.Nr.","Menge","Bezeichnung","Baugruppe","Material"]
[1,1,1,"ET1",null,"1 kg"]
[1,2,4,"FT1",null,"Best.Nr. 12345"]
[1,3,2,"ET4",null,"1 m"]

{"sheet":"S-P001","index":7,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,0,0,5]]}
["S-P001- Baugruppe"]
["Stufe","Pos.Nr.","Menge","Bezeichnung","Baugruppe","Material"]
["1","1","1","BG1","P002"]
[".2",1,1,"ET1",null,"1 kg"]
[".2",2,2,"ET2",null,"1,5 m"]
["1","2","1","BG2","P003"]
[".2",1,2,"ET1",null,"1 kg"]
[".2",2,3,"ET3",null,"2 kg"]
[".2",3,1,"BG3","P004"]
["..3",1,1,"ET1",null,"1 kg"]
["..3",2,4,"FT1",null,"Best.Nr. 12345"]
["..3",3,2,"ET4",null,"1 m"]
["1","3","2","ET3",null,"1 m"]
["1","4","1","ET4",null,"2 kg"]