{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Cover","Liste","Fehlereanalyse","74210 Code","Hanning Code","BCD Code"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":22,"n_cols":3,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Algorithmen"]
[null,"für Ingenieure"]
[]
[]
[null,"Kapitel",14]
[null,"Thema","Fehlererkennung und Fehlerkorrektur"]
[]
[null,"Inhalt","Hamming-Code"]
[]
[]
[]
[]
[]
[]
[null,"Version","1.0"]
[null,"Autor","Harald Nahrstedt"]
[null,"Datum","2025-06-14"]
[]
[]
[null,"Springer Vieweg Verlag"]

{"sheet":"Liste","index":1,"n_rows":9,"n_cols":5,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["Ziffern","Hamming-Code","Ziffern","Ziffer Nr.","Bit"]
[16548,"11010011100100010010101011001110100",16548,2,4]
[324,"100001101010001011101",324,2,1]
[33567,"10000111000011000010111001100001111",33567,4,4]
[1267389,"1101001010101011001100001100100001111100010011001",1267389,2,4]
[345,"111001110011000100100",345,2,2]
[12,"11010010101011",12,1,6]
[964,"001000111000111001100",964,3,2]
[7008,"0101111000000000000001110000",7008,4,7]

{"sheet":"Fehlereanalyse","index":2,"n_rows":9,"n_cols":5,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["P0","P1","P2","Kontrollbit","Fehlerbit"]
[0,0,0,"-","-"]
[0,0,1,"K0",1]
[0,1,0,"K1",2]
[0,1,1,"K0 & K1",3]
[1,0,0,"K2",4]
[1,0,1,"K0 & K2",5]
[1,1,0,"K1 & K2",6]
[1,1,1,"K9 & K1 & K2",7]

{"sheet":"74210 Code","index":3,"n_rows":12,"n_cols":6,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["Bit",5,4,3,2,1]
["Wert",7,4,2,1,0]
[0,1,1,0,0,0]
[1,0,0,0,1,1]
[2,0,0,1,0,1]
[3,0,0,1,1,0]
[4,0,1,0,0,1]
[5,0,1,0,1,0]
[6,0,1,1,0,0]
[7,1,0,0,0,1]
[8,1,0,0,1,0]
[9,1,0,1,0,0]

{"sheet":"Hanning Code","index":4,"n_rows":12,"n_cols":8,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["Bit",1,2,3,4,5,6,7]
["Wert","K0","K1",8,"K2",4,2,1]
[0,0,0,0,0,0,0,0]
[1,1,1,0,1,0,0,1]
[2,0,1,0,1,0,1,0]
[3,1,0,0,0,0,1,1]
[4,1,0,0,1,1,0,0]
[5,0,1,0,0,1,0,1]
[6,1,1,0,0,1,1,0]
[7,0,0,0,1,1,1,1]
[8,1,1,1,0,0,0,0]
[9,0,0,1,1,1,0,1]

{"sheet":"BCD Code","index":5,"n_rows":11,"n_cols":6,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Ziffer","23","22","21","20","Paritätsbit"]
[0,0,0,0,0,0]
[1,0,0,0,1,1]
[2,0,0,1,0,1]
[3,0,0,1,1,0]
[4,0,1,0,0,1]
[5,0,1,0,1,0]
[6,0,1,1,0,0]
[7,0,1,1,1,1]
[8,1,0,0,0,1]
[9,1,0,0,1,0]